Scaffold Pre-Use Daily Inspection

|  |  |
| --- | --- |
| Location  | Project  |
| Date Click to enter date | Time  | Scaffold Type  |
|  Inspected By (Competent Person-Scaffolding)  |

|  |  |  |
| --- | --- | --- |
| **Site Conditions** | **Yes** | **No** |
| 1 | Has work location been examined before start of work and all appropriate precautions taken? (e.g., checking for overhead objects, falling or tripping hazards, uneven ground) |[ ] [ ]
| 2 | Has the scaffold been set up according to manufacturer’s and/or design engineer’s instructions? |[ ] [ ]
| **General Requirements for All Scaffolds** | **Yes** | **No** |
| 3 | Can scaffold components support at least four times their maximum intended load? |[ ] [ ]
| 4 | Is the maximum load capacity of this scaffold known and communicated to all employees? |[ ] [ ]
| 5 | Are all platforms fully planked with scaffold grade planks in good condition and no more than 1” gap between planks?  |[ ] [ ]
| 6 | Are platforms at least 18” wide? |[ ] [ ]
| 7 | Are all platform units cleated, restrained by hooks or equivalent means, or extending over the center line of their supports by at least 6”? |[ ] [ ]
| 8 | Are guardrails (toprail, midrail, toeboard, posts) used on all open sides and ends of scaffolds over 6 ft. high? |[ ] [ ]
| 9 | Will the guardrails withstand 200 pounds in a downward or outward direction? |[ ] [ ]
| 10 | Is the front edge of platform less than 14” from face work (if guardrails removed)? |[ ] [ ]
| 11 | If scaffold components of different manufacturers are used, do they fit together without force and has a competent person determined that they are safe for use? |[ ] [ ]
| 12 | Are scaffolds, tools, and materials at least 10 ft. away from energized power lines? |[ ] [ ]
| 13 | Is platform free of clutter, mud, oil, or any tripping hazard? |[ ] [ ]
| **Supported Scaffolds** | **Yes** | **No** |
| 14 | Has the scaffold been constructed to maintain a safety factor of 4:1 height to base width ratio? |[ ] [ ]
| 15 | If ratio is more than 4:1, are scaffolds secured to a building or structure as required? |[ ] [ ]
| 16 | Is scaffold plumb, square, and level? |[ ] [ ]
| 17 | Have diagonal stiff legs and/or guy wires been installed to support the scaffold towers? |[ ] [ ]
| 18 | Are U-bolts placed over the dead end of the wire, and the saddles placed of the live end of the wire? |[ ] [ ]
| 19 | Is a guy wire installed at a horizontal member that supports the inner and outer legs? |[ ] [ ]
| 20 | Are legs, posts, frames and uprights on base plates attached to mudsills (if on dirt)? |[ ] [ ]
| 21 | Are footings level, sound, rigid, and capable of supporting 4 times the intended load without settling? |[ ] [ ]
| 22 | Are poles, legs, and uprights plumb and securely braced to prevent swaying or displacement? |[ ] [ ]
| 23 | Are scaffold components free of any bends, cracks, holes, rust, welding splatter, pits, broken welds, or non-compatible parts? |[ ] [ ]
| 24 | Unstable objects such as blocks, bricks, buckets, etc. are **not** used as work platforms or to support scaffolds. |[ ] [ ]
| **Access** | **Yes** | **No** |
| 25 | Is safe access provided for all scaffold platforms that are more than 2 ft. above or below the point of access? |[ ] [ ]
| 26 | If ladder used, is it securely attached to the scaffold and extends at least 3 ft. above the platform level? |  |  |
| **Stairway-type Ladders** | **Yes** | **No** |
| 27 | Is the bottom step no more than 24” above the scaffold supporting level and does the ladder extend 36” above the working platform? |[ ] [ ]
| 28 | Are slip-resistant treads on all steps and landings? |[ ] [ ]
| 29 | Are stair rails consisting of a top-rail and a mid-rail provided on each side of each scaffold stairway? |[ ] [ ]
| **Use** | **Yes** | **No** |
| 31 | Have all workers been properly trained by a qualified person? |[ ] [ ]
| 32 | Is scaffolding within rated capacity for loads, materials, workers and weather conditions? |[ ] [ ]
| 33 | Has the scaffold been inspected by a competent person as required? |[ ] [ ]
| 34 | If any piece of scaffold is defective, has it been removed from service and tagged? |[ ] [ ]
| **Personal Fall Protection** | **Yes** | **No** |
| 35 | Are personal fall protection systems used where guardrails are not feasible? |[ ] [ ]
| **Falling Object Protection** | **Yes** | **No** |
| 36 | Have toeboards at least 3.5“ high been installed to prevent falling objects? |[ ] [ ]
| 37 | Are screens/barriers installed between toeboard and guardrail, if objects taller than toeboards? |[ ] [ ]
| 38 | Is the area below scaffolding designated hard hat only, barricaded and posted with warning signs? |[ ] [ ]
| Comments: Click to enter text |